{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["使い方","入力フォーム","How to use","Input form","選択肢_日本語","選択肢_英語"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"使い方","index":0,"n_rows":27,"n_cols":1,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["リスク評価　一括再評価テンプレート"]
[]
["【入力ルール — 物理状態による制約】"]
["物理状態（D列）の選択値によって、入力できる列が変わります。"]
["ルールに違反した値が入力されたセルは赤く強調表示されます。"]
[]
["・固体  →  飛散性（H列）のみ入力可（揮発性・引火温度・気体区分は空白に）"]
["・液体  →  揮発性(沸点)（E列）・取扱温度（F列）のみ入力可"]
["・気体  →  気体区分（G列）・取扱温度（F列）のみ入力可"]
[]
["【使い方】"]
["1. ケミカンSDS管理からダウンロードしたCSVファイルをExcelで開いてください。"]
["2. 「入力フォーム」シートにCSVファイルの情報を貼り付けてください。"]
["3. 「入力フォーム」シートで各行の作業条件をドロップダウンから選択してください。"]
["4. SDS ID、ファイル名、製品名（グレー列）は変更しないでください。"]
["5. 赤くなったセルは物理状態と不整合です。値を削除するか物理状態を修正してください。"]
["6. 編集完了後：「ファイル」→「名前を付けて保存」→「CSV UTF-8（コンマ区切り）」で保存してください。"]
["7. 保存したCSVファイルをアップロードしてください。"]
[]
["■Excelマクロを使用する場合"]
["1. ケミカンSDS管理からダウンロードしたCSVファイルをExcelで開いてください。"]
["2. 「入力フォーム」シートにCSVファイルの情報を貼り付けてください。"]
["3. 「入力フォーム」シートで各行の作業条件をドロップダウンから選択してください。"]
["4. SDS ID、ファイル名、製品名（グレー列）は変更しないでください。"]
["5. 赤くなったセルは物理状態と不整合です。値を削除するか物理状態を修正してください。"]
["6. 編集完了後：「CSVとして保存」ボタンを押してファイルを保存してください。"]
["7. 保存したCSVファイルをアップロードしてください。"]

{"sheet":"入力フォーム","index":1,"n_rows":2,"n_cols":16,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[]
["SDS ID","ファイル名","製品名","物理状態","揮発性(沸点)","取扱温度","気体区分","飛散性","取扱量","年間作業時間","作業環境_換気_保護設備_保護具使用","作業環境_換気_保護設備_密閉化","作業環境_換気_保護設備_局所排気","作業環境_換気_保護設備_全体換気または屋外","作業環境_換気_保護設備_空気希釈","作業環境_換気_保護設備_ガス検知器"]

{"sheet":"How to use","index":2,"n_rows":27,"n_cols":1,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["Risk Assessment — Bulk Re-evaluation Template"]
[]
["[Input Rules — Constraints by Physical State]"]
["The columns you can fill in change depending on the physical state selected in Column D."]
["Cells containing values that violate the rules are highlighted in red."]
[]
["- Solid   →  Only Dustiness (Column H) can be entered (leave Volatility, Flash Point, and Gas Classification blank)"]
["- Liquid  →  Only Volatility (Boiling Point) (Column E) and Handling Temperature (Column F) can be entered"]
["- Gas     →  Only Gas Classification (Column G) and Handling Temperature (Column F) can be entered"]
[]
["[How to Use]"]
["1. Open the CSV file you downloaded from Chemican SDS Management in Excel."]
["2. Paste the contents of the CSV file into the \"Input Form\" sheet."]
["3. On the \"Input Form\" sheet, select the working conditions for each row from the dropdowns."]
["4. Do not change the SDS ID, File Name, or Product Name (the gray columns)."]
["5. Cells turned red are inconsistent with the physical state. Either delete the value or correct the physical state."]
["6. When you're done editing: \"File\" → \"Save As\" → save as \"CSV UTF-8 (Comma delimited)\"."]
["7. Upload the saved CSV file."]
[]
["■ If using the Excel macro"]
["1. Open the CSV file you downloaded from Chemican SDS Management in Excel."]
["2. Paste the contents of the CSV file into the \"Input Form\" sheet."]
["3. On the \"Input Form\" sheet, select the working conditions for each row from the dropdowns."]
["4. Do not change the SDS ID, File Name, or Product Name (the gray columns)."]
["5. Cells turned red are inconsistent with the physical state. Either delete the value or correct the physical state."]
["6. When you're done editing: click the \"Save as CSV\" button to save the file."]
["7. Upload the saved CSV file."]

{"sheet":"Input form","index":3,"n_rows":2,"n_cols":16,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[]
["SDS ID","file_name","product_name","physical_condition","volatility","operating_temperature","gas_classification","dustiness","amount","annual_operating_time","skin_protection","remote_or_enclosed_system","local_exhaust_ventilation","general_ventilation_or_outside","air_dilution","gas_detector"]

{"sheet":"選択肢_日本語","index":4,"n_rows":6,"n_cols":8,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["物理状態","揮発性","引火温度","気体区分","飛散性","取扱量","年間作業時間","あり/なし"]
["液体","沸点 50℃未満（高揮発性）","引火点以上","爆発範囲内：高圧ガス / 液化ガス","粉塵多い","グラム（少量）","400時間/年以上","あり"]
["気体","沸点 50℃以上、150℃未満（中揮発性）","引火点から−10℃以上、引火点未満","爆発範囲外","粉塵少ない","キログラム（中量）","100時間/年以上、400時間/年未満","なし"]
["固体","沸点 150℃以上（低揮発性）","引火点から−10℃未満",null,"フレーク状等","トン（大量）","25時間/年以上、100時間/年未満"]
[null,null,"引火点なし（不燃性）",null,null,null,"10時間/年以上、25時間/年未満"]
[null,null,null,null,null,null,"10時間/年未満"]

{"sheet":"選択肢_英語","index":5,"n_rows":6,"n_cols":8,"rows_kept":6,"cut":false,"hidden":true,"merged":[]}
["Physical Condition","Volatility","Operating Temperature","Explosion Range","Dustiness","Amount Handled","Annual Operating Time","Yes/No"]
["Liquid","Boiling point below 50°C (high volatility)","At or above flash point","Within explosion range: High-pressure gas / Liquefied gas","High dustiness","Gram (small quantity)","400 hours/year or more","Yes"]
["Gas","Boiling point 50°C to below 150°C (medium volatility)","Within 10°C below flash point","Outside explosion range","Low dustiness","Kilogram (medium quantity)","100-400 hours/year","No"]
["Solid","Boiling point 150°C or more (low volatility)","More than 10°C below flash point",null,"Flake-like, etc.","Ton (large quantity)","25-100 hours/year"]
[null,null,"No flash point (non-flammable)",null,null,null,"10-25 hours/year"]
[null,null,null,null,null,null,"Less than 10 hours/year"]